Professor Tina Smilkstein



EE431 [ October 7, 2021]

Austin Ma


Key binding Ctrl+A selects all of the figures in the schematic


Key binding Ctrl+D deselects all of the figures in the schematic


The lower case f key allows us to zoom the schematic to fit on screen


1. 
2. 


So 60uA seems to be the max current draw


1. 











Why does the simulation take 1 minute to do sometimes and 2 seconds to do othertimes?