EE431, Lab 4

Professor Tina Smilkstein

Austin Ma

1. 716 gates
2. Approximately 10,969.414
3. square micrometers?
4. 32.667nW of leakage power, or like 4nA for 8V of VDD
5. 2007890.157 nW of switching power
6. Switching power is about the average amount of power it takes to switch each time?
7. Maybe the worst is case a 100 to a couple hundred gates for a single path



